{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Battery_life_calc"],"not_rendered":{"charts":0,"images":16,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Battery_life_calc","index":0,"n_rows":38,"n_cols":16,"rows_kept":38,"cut":false,"hidden":false,"merged":[[3,1,3,4],[8,3,8,4],[9,3,9,4],[4,1,5,1],[4,3,4,4],[7,3,7,4],[6,3,6,4],[5,3,5,4],[0,0,1,8],[19,5,22,7],[19,2,22,4],[19,1,22,1],[2,1,2,7],[4,5,4,6],[3,5,3,7],[16,5,18,6],[15,5,15,6],[5,7,14,7],[9,1,11,1],[12,1,16,1],[2,8,25,8],[2,0,25,0],[5,5,14,6],[17,1,18,1],[12,3,12,4],[11,3,11,4],[6,1,7,1],[18,3,18,4],[23,1,25,7],[17,3,17,4],[13,2,16,2],[10,3,10,4],[16,3,16,4],[15,3,15,4],[14,3,14,4],[13,3,13,4]]}
[]
[]
[null,"Tag Battery Lifetime Estimation"]
[null,"SETTINGS",null,null,null,"Estimated lifetime"]
[null,"Tag","Tag Type","Tag Leonardo Asset",null,"Days",null,"Total Number of Blinks"]
[null,null,"FW","3.125 and newer",null,1676.7644359072567,null,72436296]
[null,"Radio","Channel",5]
[null,null,"RF profile","RF5"]
[null,"Blink","Refresh Rate [ms]","1000"]
[null,"Sleep","Sleep mode","Immediate sleep"]
[null,null,"Refresh Rate in sleep  mode [ms]","0"]
[null,null,"Motion / no motion ratio (0-1)","0.5"]
[null,"Sensors","Payload","none"]
[null,null,"Sensors data",false]
[null,null,null,false]
[null,null,null,false,null,"Avg. Current [mA]"]
[null,null,null,false,null,2.484944561942706E-2]
[null,"Battery","Battery ",false]
[null,null,"Capacity [mAh]",1000]
[]
[]
[]
[]
[null,"DISCLAIMER: In no event shall Sewio, its employees or suppliers, licensors or affiliates be liable for any lost profits, revenue or sales arising out of the use of or inability to reach estimated battery lifetime."]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"RF_profile","Sleep mode","Payload","Tag Type","FW version"]
[null,null,null,null,null,null,null,null,null,null,null,"RF4","Disabled","none","Tag Leonardo Asset","3.119 to 3.124"]
[null,null,null,null,null,null,null,null,null,null,null,"RF5","Immediate sleep","quaternion","Tag Leonardo iMU","3.125 and newer"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"RAW_data","Tag Leonardo Personal"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Piccolino Tag (CR2450)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Piccolino Tag (CR2477)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tag IMU"]